The input signal to the active suspension system is an actuation force, which is modeled by a chirp signal. The system outputs are time, four system states, actuation force and acceleration. Four states are the travel of the top plate and the middle plate and their derivatives. Displacements are measured by the encoder.

Matlab Code for Data separation is attached:

